(module Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 58705FA3)
  (descr "Through hole pin header, pitch 1.27mm")
  (tags "pin header")
  (fp_text reference REF** (at -1.8 0 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PH2X05VR1MM27 (at 0 6.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.1 0.5) (end -1.1 -1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 -1.1) (end 0.5 -1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 -0.8) (end 1.3 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 5.85) (end 2.1 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 5.85) (end -0.85 5.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 -1.05) (end -1.1 6.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.35 -1.05) (end 2.35 6.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.1 -1.05) (end 2.35 -1.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.1 6.1) (end 2.35 6.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.85 5.85) (end -0.85 1.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.5 -0.8) (end -0.85 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.85 -0.8) (end -0.85 0.5) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 0 1.27) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 0 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at 0 3.81) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole circle (at 0 5.08) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 1.27 1.27) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 1.27 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at 1.27 3.81) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at 1.27 5.08) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 1.27 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
)
