(module Buttons_Switches_ThroughHole:SW_Tactile_SKHH_Angled (layer F.Cu) (tedit 58FF2BB1)
  (descr "tactile switch 6mm ALPS SKHH right angle http://www.alps.com/prod/info/E/HTML/Tact/SnapIn/SKHH/SKHHLUA010.html")
  (tags "tactile switch 6mm ALPS SKHH right angle")
  (fp_text reference S1 (at 0.7 7.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
  )
  (fp_text value SW_PBTN_2PIN_V (at 2.65 -5.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.3 -4.3) (end 7.2 -4.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.2 -4.3) (end 7.2 -1.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.2 -1.1) (end 6.1 -1.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.1 -1.1) (end 6.1 2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.2 -4.3) (end -2.7 -4.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.7 -4.3) (end -2.7 -1.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.7 -1.1) (end -1.6 -1.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.6 -1.1) (end -1.6 2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.3 -2.3) (end 0.2 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.6 2.9) (end 0.3 2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.3 2.9) (end 0.3 6.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.3 6.2) (end 4.2 6.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.2 6.2) (end 4.2 2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.2 2.9) (end 6.1 2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.3 -4.3) (end 4.3 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.2 -2.3) (end 0.2 -4.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.92 5.85) (end 0.58 5.85) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 2.55) (end -1.25 -4) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 -4) (end -0.85 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 5.35 -4) (end 5.75 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 5.75 -4) (end 5.75 2.55) (layer F.Fab) (width 0.1))
  (fp_line (start -0.85 -2) (end 5.35 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.85 -2) (end -0.85 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 5.35 -2) (end 5.35 -4) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 2.55) (end 0.58 2.55) (layer F.Fab) (width 0.1))
  (fp_line (start 0.58 2.55) (end 3.92 2.55) (layer F.Fab) (width 0.1))
  (fp_line (start 3.92 2.55) (end 5.75 2.55) (layer F.Fab) (width 0.1))
  (fp_line (start 3.92 2.55) (end 3.92 5.85) (layer F.Fab) (width 0.1))
  (fp_line (start 0.58 2.55) (end 0.58 5.85) (layer F.Fab) (width 0.1))
  (fp_line (start -1.45 -1) (end -1.45 2.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.25 2.75) (end 5.75 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.95 2.55) (end 5.95 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.25 -2.2) (end 0.25 -2.2) (layer F.SilkS) (width 0.12))
  (fp_circle (center 4.5 0) (end 4.9445 0) (layer F.Mask) (width 0))
  (fp_circle (center 0 0) (end 0.4445 0) (layer F.Mask) (width 0))
  (fp_circle (center -1.25 -2.5) (end -0.615 -2.5) (layer F.Mask) (width 0))
  (fp_circle (center 5.75 -2.5) (end 6.385 -2.5) (layer F.Mask) (width 0))
  (fp_circle (center -1.25 -2.5) (end -0.107 -2.5) (layer B.Mask) (width 0))
  (fp_circle (center 4.5 0) (end 5.389 0) (layer B.Mask) (width 0))
  (fp_circle (center 0 0) (end 0.889 0) (layer B.Mask) (width 0))
  (fp_circle (center 5.75 -2.5) (end 6.893 -2.5) (layer B.Mask) (width 0))
  (pad 3 thru_hole circle (at -1.25 -2.5) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 5.75 -2.5) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 4.5 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
)
