(module DO-214AB (layer F.Cu) (tedit 5825692F)
  (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
  (tags "DO-214AB diode")
  (attr smd)
  (fp_text reference REF** (at 0 -4.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DO-214AB (at 0 4.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -5.5 -2.6) (end -5.5 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.15 -3.45) (end 5.15 -3.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.15 -3.45) (end 5.15 3.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.15 3.45) (end -5.15 3.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.15 3.45) (end -5.15 -3.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.5 3.2) (end -4.8 3.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.8 -3.2) (end 3.5 -3.2) (layer F.SilkS) (width 0.15))
  (pad 2 smd rect (at 3.6 0) (size 2.6 3.2) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.6 0) (size 2.6 3.2) (layers F.Cu F.Paste F.Mask))
  (model Diodes_SMD.3dshapes/DO-214AB.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.39 0.39 0.39))
    (rotate (xyz 0 0 180))
  )
)
