(module relay_9001 (layer F.Cu) (tedit 58F9BC5C)
  (descr "relay, Coto 9001 series Reed")
  (fp_text reference RLY*** (at 0 -4.1) (layer F.SilkS)
    (effects (font (thickness 0.3048)))
  )
  (fp_text value relay_9001 (at 0 4.3) (layer F.SilkS)
    (effects (font (thickness 0.3048)))
  )
  (fp_line (start -8.6 -3) (end -8.6 3) (layer F.SilkS) (width 0.3048))
  (fp_line (start 0.8 0) (end 2.5 0) (layer F.SilkS) (width 0.3048))
  (fp_line (start -2.5 0) (end -0.8 0) (layer F.SilkS) (width 0.3048))
  (fp_line (start -0.8 0.8) (end 0.8 -0.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start -0.8 -0.8) (end 0.8 -0.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start 0.8 -0.8) (end 0.8 0.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start -0.8 0.8) (end 0.8 0.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start -0.8 0.8) (end -0.8 -0.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start 1.5 -1.8) (end 7.6 -1.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start 7.6 -1.8) (end 7.6 0) (layer F.SilkS) (width 0.3048))
  (fp_line (start -7.6 -1.8) (end -7.6 0) (layer F.SilkS) (width 0.3048))
  (fp_line (start -7.6 -1.8) (end -1.1 -1.8) (layer F.SilkS) (width 0.3048))
  (fp_line (start -1.1 -1.8) (end 1.5 -2.3) (layer F.SilkS) (width 0.3048))
  (fp_line (start 10.3 -3) (end 10.3 3) (layer F.SilkS) (width 0.3048))
  (fp_line (start -10.3 -3) (end -10.3 3) (layer F.SilkS) (width 0.3048))
  (fp_line (start -10.3 3) (end 10.3 3) (layer F.SilkS) (width 0.3048))
  (fp_line (start -10.3 -3) (end 10.3 -3) (layer F.SilkS) (width 0.3048))
  (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 7.62 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -7.62 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (model walter/relay/relay_9001.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
