(footprint "VPR221_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 3.81 -23.42) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cd59375d-9055-4dc3-bdd7-7cd89c1487b3)
  )
  (fp_text value "VPR221_Horizontal" (at 3.81 2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e5043a76-4e11-4140-b80b-bc311cdd8dd0)
  )
  (fp_text user "${REFERENCE}" (at 3.81 -23.42) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f501908f-978e-4a4d-b027-ed72be7b9352)
  )
  (fp_line (start -1.31 -22.42) (end -1.31 -6.53)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef5e1460-7abf-44fb-b2e2-0bf72ef2dcdd))
  (fp_line (start -1.31 -22.42) (end 8.93 -22.42)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fb5527aa-e58b-4cfb-8bf5-a30f4ded5452))
  (fp_line (start -1.31 -6.53) (end 8.93 -6.53)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1670f622-3a73-4e9d-832c-dfb8f1693b88))
  (fp_line (start 0 -6.5) (end 0 -1.15)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2177bd24-d46e-4cb6-a663-ec185cc72e00))
  (fp_line (start 2.54 -6.5) (end 2.54 -1.15)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 819c82d4-09d7-4237-abb8-ec7fa4a08855))
  (fp_line (start 5.08 -6.5) (end 5.08 -1.15)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d06d308-95eb-44f7-9600-23e12d52f0d8))
  (fp_line (start 7.62 -6.5) (end 7.62 -1.15)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 551cb2e2-9d4f-4e89-9c53-220df6a1dc3b))
  (fp_line (start 8.93 -22.42) (end 8.93 -6.53)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5739c00e-2924-4f5c-bc94-6c0b56147cf6))
  (fp_line (start -1.44 -22.55) (end -1.44 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c7cc5618-f1fa-4090-ba53-65b555568e17))
  (fp_line (start -1.44 1.25) (end 9.06 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 79790b37-d8f1-4a67-a0a4-9bed4574ef35))
  (fp_line (start 9.06 -22.55) (end -1.44 -22.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3ec90a0f-a92b-4990-aec9-eb896d0d5346))
  (fp_line (start 9.06 1.25) (end 9.06 -22.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e560da81-ae80-4b32-bb3b-4164595f1cee))
  (fp_line (start -1.19 -22.3) (end 8.81 -22.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0c141ae0-bdf4-4c9c-9f70-05fc2a68cbe5))
  (fp_line (start -1.19 -15.9) (end -1.19 -22.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cef8294d-2ed0-4606-b487-4c96544f9f66))
  (fp_line (start -1.19 -15.9) (end 8.81 -15.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c0fcbe1-46b9-4b02-8bda-db08f28ba8ff))
  (fp_line (start -1.19 -6.65) (end -1.19 -15.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9421d99-82ac-4b88-99fe-863ada55f04b))
  (fp_line (start 0 -6.6) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91920da3-3770-4025-a91e-2aac48e1d365))
  (fp_line (start 2.54 -6.6) (end 2.54 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ceb625b9-25af-4fd9-a936-f2c1bf00d25f))
  (fp_line (start 5.08 -6.6) (end 5.08 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0c01ed7a-bab9-4bef-8001-1160d0232339))
  (fp_line (start 7.62 -6.6) (end 7.62 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69e6f578-a0a4-4c13-b218-baee7955a43f))
  (fp_line (start 8.81 -22.3) (end 8.81 -15.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e64fdb8f-826e-4bc8-afae-dc7684ff9474))
  (fp_line (start 8.81 -15.9) (end -1.19 -15.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc7ee587-464e-4f4e-8352-0fb027359bbe))
  (fp_line (start 8.81 -15.9) (end 8.81 -6.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4511d1d9-1101-4664-9514-8edb7d678b90))
  (fp_line (start 8.81 -6.65) (end -1.19 -6.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5777baf1-99f6-45a6-a54f-f902369c5a58))
  (fp_circle (center 3.81 -19.5) (end 5.66 -19.5)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 64b2e857-0947-4888-b3b0-c586b1bb1fbf))
  (pad "" np_thru_hole oval (at 3.81 -19.5) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp b1e96885-9b41-46d1-b103-6ba9d8a0b754))
  (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 0310291c-f5d7-4d4f-8538-0bf4dfbaa16c))
  (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 41122df6-d4fa-48c0-911e-6b1615d01fba))
  (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp b72019fc-c972-483b-86d7-984ddcf620d0))
  (pad "4" thru_hole oval (at 7.62 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 3c57db2d-c55c-4a08-9b12-ffdae412317c))
  (model "${KIPRJMOD}/kirdy.pretty/VPR221_Horizontal.step"
    (offset (xyz 3.75 14.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
