(footprint "LD_Heat_Sink" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 2 -0.8 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp b03508c4-b870-4a6c-8081-4a3172acbcc5)
  )
  (fp_text value "LD_Heat_Sink" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a0fa68b9-ef2c-4687-87d4-aebc85f361b1)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ee47ee06-c924-4e15-a665-2f893aaca683)
  )
  (fp_line (start 0 0) (end 0 43.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp e1b2467a-849d-45b9-9f3c-2685c4dcd8ac))
  (fp_line (start 0 43.2) (end 13.237 43.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp ec212cd5-00bf-4133-bc26-ccbe54309d25))
  (fp_line (start 13.237 43.2) (end 13.237 50)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp f98ebb46-3a1d-48d5-ba63-983b16cc7581))
  (fp_line (start 13.237 50) (end 85 50)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 66a57136-02b2-47f9-b55f-8e94953b2188))
  (fp_line (start 20 0) (end 0 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 799c80cf-38f7-4367-8431-d21acddd9ca6))
  (fp_line (start 20 38.8) (end 20 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 8ebe8182-cf22-4829-b4fb-e4da639edc80))
  (fp_line (start 33.86 0) (end 33.86 38.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c8334ace-8dc2-4a3a-9b5f-eb043a943919))
  (fp_line (start 33.86 38.8) (end 20 38.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 93634a35-66a4-483e-9033-a37c80573ec6))
  (fp_line (start 51.14 0) (end 33.86 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3e107afb-3bce-4862-bdfe-43be8f99d27a))
  (fp_line (start 51.14 38.8) (end 51.14 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7d78005b-79e2-4ed1-8c95-c6e6377aade7))
  (fp_line (start 65 0) (end 65 38.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7e8e8b21-d486-454f-976e-c47119a42e6c))
  (fp_line (start 65 38.8) (end 51.14 38.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp a4698f07-e62f-4085-9224-6e739071ad77))
  (fp_line (start 85 0) (end 65 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 632100a3-370a-4dd3-b967-0b46b613d56f))
  (fp_line (start 85 50) (end 85 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c4a85d4c-95f9-4ca5-9166-a7ed4eb818d5))
  (model "${KIPRJMOD}/laserSocket.pretty/kirdy_LD_adapter_copper_plate.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
