(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "+18V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "#PWR" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value" "+18V" (at 0 3.556 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "power-flag" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power symbol creates a global label with name \"+18V\"" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "+18V_0_1"
      (polyline
        (pts
          (xy -0.762 1.27)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 0)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0.762 1.27)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "+18V_1_1"
      (pin power_in line (at 0 0 90) (length 0) hide
        (name "+1V8" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "AD5680" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AD5680" (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (at -8.89 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad5680.pdf" (at -8.89 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD5680_0_0"
      (pin power_in line (at 8.89 12.7 180) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 12.7 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 7.62 180) (length 2.54)
        (name "VFB" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 10.16 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 7.62 0) (length 2.54)
        (name "~{SYNC}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 5.08 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 2.54 0) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 2.54 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AD5680_0_1"
      (rectangle (start -6.35 15.24) (end 6.35 0)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "AD7172-2" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 8.89 -22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AD7172-2" (at -6.35 -22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (at 2.54 -25.4 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad7172-2.pdf" (at 46.99 -46.99 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "24 bit precision ADC" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD7172-2_0_0"
      (pin input line (at -13.97 1.27 0) (length 2.54)
        (name "AIN4" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 21.59 180) (length 2.54)
        (name "XTAL2/CLKIO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 13.97 16.51 180) (length 2.54)
        (name "DOUT/~{RDY}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 13.97 180) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 11.43 180) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 8.89 180) (length 2.54)
        (name "~{CS}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 6.35 180) (length 2.54)
        (name "~{SYNC}/~{ERR}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -8.89 180) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -19.05 180) (length 2.54)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 13.97 -3.81 180) (length 2.54)
        (name "REGCAPD" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 1.27 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 21.59 0) (length 2.54)
        (name "REF-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 -1.27 180) (length 2.54)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 11.43 0) (length 2.54)
        (name "AIN0" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 8.89 0) (length 2.54)
        (name "AIN1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 6.35 0) (length 2.54)
        (name "AIN2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 3.81 0) (length 2.54)
        (name "AIN3" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 24.13 0) (length 2.54)
        (name "REF+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -13.97 19.05 0) (length 2.54)
        (name "REFOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -13.97 -3.81 0) (length 2.54)
        (name "REGCAPA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -19.05 0) (length 2.54)
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -8.89 0) (length 2.54)
        (name "AVDD1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -11.43 0) (length 2.54)
        (name "AVDD2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 24.13 180) (length 2.54)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AD7172-2_0_1"
      (rectangle (start -11.43 26.67) (end 11.43 -21.59)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "AD7172-4BCPZ" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 33.02 -49.53 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "AD7172-4BCPZ" (at 5.08 -49.53 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "kirdy:QFN50P500X500X80-33N-D" (at 36.83 -87.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://componentsearchengine.com/Datasheets/2/AD7172-4BCPZ.pdf" (at 36.83 -187.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "MFR_PN" "AD7172-4BCPZ" (at 36.83 -787.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "ANALOG DEVICES - AD7172-4BCPZ - Analogue to Digital Converter, Sigma-Delta, 24 bit, 31.25 kSPS, Differential, Single Ended, SPI" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD7172-4BCPZ_1_1"
      (rectangle (start 5.08 2.54) (end 35.56 -48.26)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at 0 -6.35 0) (length 5.08)
        (name "AIN0/REF2-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -2.54 180) (length 5.08)
        (name "XTAL2/CLKIO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 -6.35 180) (length 5.08)
        (name "DOUT/~{RDY}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 40.64 -8.89 180) (length 5.08)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 40.64 -11.43 180) (length 5.08)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 40.64 -13.97 180) (length 5.08)
        (name "~{CS}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -16.51 180) (length 5.08)
        (name "~{ERROR}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 40.64 -19.05 180) (length 5.08)
        (name "~{SYNC}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -36.83 180) (length 5.08)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -43.18 180) (length 5.08)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 -33.02 180) (length 5.08)
        (name "REGCAPD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -8.89 0) (length 5.08)
        (name "AIN1/REF2+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -22.86 180) (length 5.08)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -25.4 180) (length 5.08)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -27.94 180) (length 5.08)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -11.43 0) (length 5.08)
        (name "AIN2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -13.97 0) (length 5.08)
        (name "AIN3" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -16.51 0) (length 5.08)
        (name "AIN4" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -19.05 0) (length 5.08)
        (name "AIN5" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -21.59 0) (length 5.08)
        (name "AIN6" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -24.13 0) (length 5.08)
        (name "AIN7" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -26.67 0) (length 5.08)
        (name "AIN8" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 40.64 -39.37 180) (length 5.08) hide
        (name "DNC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 -30.48 180) (length 5.08)
        (name "GPO3" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -2.54 0) (length 5.08)
        (name "REF-" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 0 0) (length 5.08)
        (name "REF+" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -45.72 180) (length 5.08)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -30.48 0) (length 5.08)
        (name "REGCAPA" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -45.72 0) (length 5.08)
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -36.83 0) (length 5.08)
        (name "AVDD1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -39.37 0) (length 5.08)
        (name "AVDD2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -33.02 0) (length 5.08)
        (name "PDSW" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 0 180) (length 5.08)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ADP150AUJZ-3.3" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ADP150AUJZ-3.3" (at -7.62 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adp150.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low noise LDO" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ADP150AUJZ-3.3_0_0"
      (pin power_in line (at 5.08 10.16 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 5.08 7.62 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 13.97 8.89 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 10.16 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ADP150AUJZ-3.3_0_1"
      (rectangle (start 7.62 12.7) (end 20.32 0)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start 20.32 3.81) (end 20.32 3.81)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
  )
  (symbol "AG5300" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.35 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AG5300" (at -2.54 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:AG5300" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://silvertel.com/images/datasheets/Ag5300-datasheet-smallest-30W-Power-Over-Ethernet-Plus-Module-PoEplusPD.pdf" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "PoE" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PoE Module, 12V, 30W" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AG5300_0_0"
      (pin power_in line (at -8.89 7.62 0) (length 2.54)
        (name "VIN+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -2.54 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 -2.54 0) (length 2.54)
        (name "VIN-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -8.89 2.54 0) (length 2.54)
        (name "AT-DET" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -0.635 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0.635 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 1.905 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 7.62 180) (length 2.54)
        (name "+VDC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 3.81 180) (length 2.54)
        (name "ADJ" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AG5300_0_1"
      (rectangle (start -6.35 10.16) (end 7.62 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "BG050-10A-0-0450-0737-0350-L-D" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical_SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "BG050-10A-0-0450-0737-0350-L-D" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BG050-10A-0-0450-0737-0350-L-D_1_1"
      (rectangle (start 3.81 -10.033) (end 4.445 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 4.445 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 4.445 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 4.445 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 4.445 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 1.27) (end 8.89 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 8.255 -10.033) (end 8.89 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 -7.493) (end 8.89 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 -4.953) (end 8.89 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 -2.413) (end 8.89 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 0.127) (end 8.89 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at 0 0 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -10.16 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 0 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -2.54 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -5.08 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -7.62 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -10.16 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Filter_EMI_LL_1423" (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "FL" (at 0 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Filter_EMI_LL_1423" (at 0 -4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB" (at 0 1.016 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 1.016 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "EMI filter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "EMI 2-inductor filter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "L_* L_CommonMode*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Filter_EMI_LL_1423_0_1"
      (circle (center -3.048 -1.27) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type outline))
      )
      (circle (center -3.048 1.524) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type outline))
      )
      (arc (start -2.54 2.032) (mid -2.032 1.5262) (end -1.524 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -1.524 -2.032) (mid -2.032 -1.5262) (end -2.54 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -1.524 2.032) (mid -1.016 1.5262) (end -0.508 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -0.508 -2.032) (mid -1.016 -1.5262) (end -1.524 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -0.508 2.032) (mid 0 1.5262) (end 0.508 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.032)
          (xy -2.54 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 0.508)
          (xy 2.54 0.508)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 2.032)
          (xy -2.54 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -2.032)
          (xy 2.54 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -0.508)
          (xy -2.54 -0.508)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 2.54 2.032)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 0.508 -2.032) (mid 0 -1.5262) (end -0.508 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 0.508 2.032) (mid 1.016 1.5262) (end 1.524 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 1.524 -2.032) (mid 1.016 -1.5262) (end 0.508 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 1.524 2.032) (mid 2.032 1.5262) (end 2.54 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 2.54 -2.032) (mid 2.032 -1.5262) (end 1.524 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "Filter_EMI_LL_1423_1_1"
      (pin passive line (at -5.08 2.54 0) (length 2.54)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 2.54 180) (length 2.54)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -2.54 180) (length 2.54)
        (name "3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -2.54 0) (length 2.54)
        (name "4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Kirdy_Adapter_HDR1" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BG050-10A-0-0650-0737-0350-L-D" (at 10.16 -12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:BG050-10A-0-0650-0737-0350-L-D" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "BG050-10A-0-0650-0737-0350-L-D" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Kirdy_Adapter_HDR1_1_1"
      (rectangle (start 3.81 -10.033) (end 4.445 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 4.445 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 4.445 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 4.445 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 4.445 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 1.27) (end 16.51 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 15.875 -10.033) (end 16.51 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -7.493) (end 16.51 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -4.953) (end 16.51 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -2.413) (end 16.51 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 0.127) (end 16.51 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at 0 0 0) (length 3.81)
        (name "TEC+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -10.16 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 0 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 0) (length 3.81)
        (name "TEC-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -2.54 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -5.08 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 0) (length 3.81)
        (name "NTC+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -7.62 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -10.16 0) (length 3.81)
        (name "NTC-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Kirdy_Adapter_HDR2" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BG050-10A-0-0650-0737-0350-L-D" (at 10.16 -12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:BG050-10A-0-0650-0737-0350-L-D" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "BG050-10A-0-0650-0737-0350-L-D" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Kirdy_Adapter_HDR2_1_1"
      (rectangle (start 3.81 -10.033) (end 4.445 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 4.445 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 4.445 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 4.445 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 4.445 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 1.27) (end 16.51 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 15.875 -10.033) (end 16.51 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -7.493) (end 16.51 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -4.953) (end 16.51 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -2.413) (end 16.51 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 0.127) (end 16.51 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at 0 0 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -10.16 180) (length 3.81)
        (name "LD+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 0 180) (length 3.81)
        (name "PD-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -2.54 180) (length 3.81)
        (name "PD+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -5.08 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -7.62 180) (length 3.81)
        (name "LD-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -10.16 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Kirdy_LD_Adapter" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at -6.35 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Kirdy_LD_Adapter" (at 1.27 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:Kirdy_LD_Adapter" (at -5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at -5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "Kirdy_LD_Adapter_PCB" (at 1.27 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "connector" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Kirdy_LD_Adapter 3D Model and Header Pitch Position" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Kirdy_LD_Adapter_1_1"
      (rectangle (start -7.62 1.27) (end 10.16 -1.27)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "LAN8742A" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LAN8742A" (at 0 -27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (at 0 -33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/8742a.pdf" (at 2.54 -35.56 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LAN8742A_0_0"
      (pin power_in line (at 10.16 -7.62 180) (length 2.54)
        (name "VDD2A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "RXER" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 0 0) (length 2.54)
        (name "CRS_DV" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
        (name "MDIO" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "MDC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 -15.24 0) (length 2.54)
        (name "nINT" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 2.54)
        (name "nRST" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 20.32 0) (length 2.54)
        (name "TXEN" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "TXD0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 15.24 0) (length 2.54)
        (name "TXD1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VDD1A" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "LED2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 17.78 180) (length 2.54)
        (name "TXN" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 20.32 180) (length 2.54)
        (name "TXP" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 12.7 180) (length 2.54)
        (name "RXN" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 15.24 180) (length 2.54)
        (name "RXP" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "RBIAS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -22.86 180) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "LED1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 2.54)
        (name "XTAL2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -22.86 0) (length 2.54)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -12.7 180) (length 2.54)
        (name "VDDCR" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 7.62 0) (length 2.54)
        (name "RXD1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 10.16 0) (length 2.54)
        (name "RXD0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -10.16 180) (length 2.54)
        (name "VDDIO" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LAN8742A_0_1"
      (rectangle (start -10.16 22.86) (end 7.62 -25.4)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "LT3081xDF" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LT3081xDF" (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 30.48 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 30.48 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LT3081xDF_0_0"
      (pin power_out line (at 10.16 2.54 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54) hide
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54) hide
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54) hide
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 0 180) (length 2.54)
        (name "ILIM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 0 0) (length 2.54)
        (name "SET" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -8.89 -2.54 0) (length 2.54)
        (name "IMON" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "TEMP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LT3081xDF_0_1"
      (rectangle (start -6.35 5.08) (end 7.62 -5.08)
        (stroke (width 0.1524) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "LTC3261" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LTC3261" (at 0 -13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3261fb.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC3261_0_0"
      (pin no_connect line (at 0 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 3.81 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 1.27 180) (length 2.54)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 -8.89 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 3.81 180) (length 2.54)
        (name "RT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -1.27 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 8.89 6.35 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -8.89 0) (length 2.54)
        (name "C-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -3.81 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -1.27 0) (length 2.54)
        (name "C+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 6.35 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LTC3261_0_1"
      (rectangle (start -5.08 8.89) (end 6.35 -11.43)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start 48.26 -19.05) (end 48.26 -19.05)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (rectangle (start 48.26 -19.05) (end 48.26 -19.05)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (rectangle (start 48.26 -19.05) (end 48.26 -19.05)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
  )
  (symbol "LTC6655" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LTC6655" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:LCC127P500X500X155-8N" (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc6655-6655ln.pdf" (at -1.27 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "reference" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision series voltage reference" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC6655_0_0"
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "~{SHDN}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 2.54 180) (length 2.54)
        (name "VOUT_S" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 5.08 180) (length 2.54)
        (name "VOUT_F" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LTC6655_0_1"
      (rectangle (start -7.62 7.62) (end 8.89 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "M20-8760542" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "M20-8760542" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:M20-8760542" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "M20-8760542" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "M20-8760542_1_1"
      (rectangle (start 3.81 -10.033) (end 4.445 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 4.445 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 4.445 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 4.445 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 4.445 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 1.27) (end 8.89 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 8.255 -10.033) (end 8.89 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 -7.493) (end 8.89 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 -4.953) (end 8.89 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 -2.413) (end 8.89 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 8.255 0.127) (end 8.89 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at 0 0 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -10.16 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 0 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -2.54 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -5.08 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -7.62 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -10.16 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX1968xUI" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX1968xUI" (at 5.08 16.51 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm" (at 0 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1968-MAX1969.pdf" (at 0 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "thermoelectric cooler" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power Driver for Peltier TEC Modules, +-3A, HTSSOP-28" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX1968xUI_0_1"
      (rectangle (start -7.62 15.24) (end 7.62 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "MAX1968xUI_1_1"
      (pin power_in line (at 0 17.78 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -7.62 180) (length 2.54) hide
        (name "LX2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 17.78 270) (length 2.54) hide
        (name "PVDD2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "FREQ" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -12.7 0) (length 2.54)
        (name "ITEC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -5.08 180) (length 2.54)
        (name "OS2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 0 180) (length 2.54)
        (name "OS1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 2.54 180) (length 2.54)
        (name "CS" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "~{SHDN}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 17.78 270) (length 2.54)
        (name "PVDD1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 5.08 180) (length 2.54)
        (name "LX1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 17.78 270) (length 2.54) hide
        (name "PVDD1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54) hide
        (name "LX1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -17.78 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54) hide
        (name "LX1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -17.78 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -10.16 0) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "MAXIN" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "MAXIP" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "MAXV" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -17.78 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "CTLI" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 2.54 0) (length 2.54)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -17.78 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -7.62 180) (length 2.54)
        (name "LX2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -17.78 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -7.62 180) (length 2.54) hide
        (name "LX2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 17.78 270) (length 2.54)
        (name "PVDD2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "PM1202" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.35 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PM1202" (at -2.54 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:PM1202" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.sdapo.net/product/product-12-386.html" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "PM1202" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "PoE" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PoE Module, 12V, 30W" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PM1202_0_0"
      (pin no_connect line (at -1.27 -11.43 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 5.08 180) (length 2.54)
        (name "+VDC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -1.27 -8.89 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -2.54 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 7.62 180) (length 2.54)
        (name "+VDC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "PM1202_0_1"
      (rectangle (start -6.35 10.16) (end 7.62 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
    (symbol "PM1202_1_0"
      (pin power_in line (at -8.89 7.62 0) (length 2.54)
        (name "VA1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 5.08 0) (length 2.54)
        (name "VA2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 0 0) (length 2.54)
        (name "VB1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 -2.54 0) (length 2.54)
        (name "VB2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "PM1202_1_1"
      (polyline
        (pts
          (xy 0 8.89)
          (xy 0 -3.81)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
    )
  )
  (symbol "Panel" (in_bom yes) (on_board yes)
    (property "Reference" "MH" (at 1.27 3.175 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Kirdy Front Panel" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Footprint" "kirdy:Panel" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "Kirdy Front Panel" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Kirdy Front Panel" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Panel_1_1"
      (rectangle (start 0 0) (end 12.7 -3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (text "Front Panel" (at 6.35 -1.905 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "Panel_2_1"
      (circle (center 0 0) (radius 1.27)
        (stroke (width 1.27) (type default))
        (fill (type none))
      )
      (pin input line (at 3.81 0 180) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "Panel_3_1"
      (circle (center 0 0) (radius 1.27)
        (stroke (width 1.27) (type default))
        (fill (type none))
      )
      (pin input line (at 3.81 0 180) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RJ45_ARJM11C7-114-BA-EW2" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 1.27 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "ARJM11C7-114-BA-EW2" (at 24.13 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "kirdy:ARJM11C7-114-BA-EW2_ABR" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "ARJM11C7-114-BA-EW2" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "MFR_PN" "ARJM11C7-114-BA-EW2" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RJ45, ARJM11C7-114-BA-EW2" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RJ45 Base100T PoE" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ARJM11C7-114-BA-EW2_ABR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RJ45_ARJM11C7-114-BA-EW2_0_0"
      (polyline
        (pts
          (xy 17.272 -34.544)
          (xy 16.002 -34.544)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.272 -33.909)
          (xy 16.002 -33.909)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 19.05 -34.544)
          (xy 17.78 -34.544)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 19.05 -33.909)
          (xy 17.78 -33.909)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -36.83)
          (xy 2.921 -36.83)
          (xy 2.921 -36.322)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy 2.921 -6.35)
          (xy 2.921 -5.842)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.921 -34.925)
          (xy 2.921 -34.29)
          (xy 0 -34.29)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.921 -4.445)
          (xy 2.921 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 16.637 -38.481)
          (xy 16.637 -39.116)
          (xy 18.542 -39.116)
          (xy 18.542 -38.481)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (text "C1" (at 23.749 -9.525 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C1" (at 33.02 -10.795 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C2" (at 23.749 -13.335 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C3" (at 23.749 -17.145 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C4" (at 23.749 -10.795 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C5" (at 23.749 -12.065 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C6" (at 23.749 -20.955 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C7" (at 23.749 -18.415 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "C8" (at 23.749 -19.685 0)
        (effects (font (size 0.889 0.889)))
      )
      (text "RCV" (at 8.89 -22.86 0)
        (effects (font (size 1.016 1.016)) (justify left))
      )
      (text "XMIT" (at 8.89 -15.24 0)
        (effects (font (size 1.016 1.016)) (justify left))
      )
    )
    (symbol "RJ45_ARJM11C7-114-BA-EW2_0_1"
      (polyline
        (pts
          (xy 6.35 -31.75)
          (xy 20.447 -31.75)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 -29.21)
          (xy 19.304 -29.21)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 -26.67)
          (xy 16.637 -26.67)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 -24.13)
          (xy 18.415 -24.13)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.7337 -21.59)
          (xy 6.0987 -21.59)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.7337 -19.05)
          (xy 6.0987 -19.05)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.7337 -16.51)
          (xy 6.0987 -16.51)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.7337 -13.97)
          (xy 6.0987 -13.97)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.7337 -11.43)
          (xy 6.0987 -11.43)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.7337 -8.89)
          (xy 6.0987 -8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 12.7 -20.955)
          (xy 22.733 -20.955)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 12.7 -13.335)
          (xy 22.733 -13.335)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 12.7 -9.525)
          (xy 22.733 -9.525)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 12.827 -17.145)
          (xy 22.733 -17.145)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 16.637 -35.433)
          (xy 16.637 -34.671)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 16.637 -33.909)
          (xy 16.637 -19.05)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 16.637 -19.05)
          (xy 8.89 -19.05)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 18.415 -35.433)
          (xy 18.415 -34.671)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 18.415 -33.909)
          (xy 18.415 -11.43)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 18.415 -24.13)
          (xy 18.415 -24.13)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 18.415 -11.43)
          (xy 8.89 -11.43)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 19.304 -11.43)
          (xy 19.304 -29.21)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 20.447 -19.05)
          (xy 20.447 -31.75)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 21.59 -19.685)
          (xy 21.59 -18.415)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 21.59 -19.05)
          (xy 20.447 -19.05)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 21.59 -12.065)
          (xy 21.59 -10.795)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 21.59 -11.43)
          (xy 19.304 -11.43)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 22.733 -19.685)
          (xy 21.59 -19.685)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 22.733 -18.415)
          (xy 21.59 -18.415)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 22.733 -12.065)
          (xy 21.59 -12.065)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 22.733 -10.795)
          (xy 21.59 -10.795)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 34.4805 -19.6215)
          (xy 35.7505 -19.6215)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 34.4805 -18.3515)
          (xy 35.7505 -18.3515)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 34.4805 -10.7315)
          (xy 35.7505 -10.7315)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 35.7505 -17.0815)
          (xy 34.4805 -17.0815)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 35.7505 -15.8115)
          (xy 34.4805 -15.8115)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 35.7505 -14.5415)
          (xy 34.4805 -14.5415)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 35.7505 -13.2715)
          (xy 34.4805 -13.2715)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 35.7505 -12.0015)
          (xy 34.4805 -12.0015)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 8.89 -16.51)
          (xy 10.16 -16.51)
          (xy 10.16 -17.145)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 8.89 -8.89)
          (xy 10.16 -8.89)
          (xy 10.16 -9.525)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -20.955)
          (xy 10.16 -21.59)
          (xy 8.89 -21.59)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -13.335)
          (xy 10.16 -13.97)
          (xy 8.89 -13.97)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 38.1 -40.64)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (circle (center 16.637 -26.67) (radius 0.127)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 18.415 -24.13) (radius 0.127)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "RJ45_ARJM11C7-114-BA-EW2_1_0"
      (text "1000pF" (at 13.97 -34.29 0)
        (effects (font (size 0.635 0.635)))
      )
      (text "1000pF" (at 21.59 -34.29 0)
        (effects (font (size 0.635 0.635)))
      )
    )
    (symbol "RJ45_ARJM11C7-114-BA-EW2_1_1"
      (polyline
        (pts
          (xy 3.6576 -34.798)
          (xy 2.1336 -34.798)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.683 -34.798)
          (xy 2.159 -34.798)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.683 -4.318)
          (xy 2.159 -4.318)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.5466 -34.925)
          (xy 4.5466 -35.179)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.572 -4.445)
          (xy 4.572 -4.699)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.8006 -35.56)
          (xy 4.8006 -35.814)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.826 -5.08)
          (xy 4.826 -5.334)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.8054 -40.64)
          (xy 17.8054 -39.116)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.0386 -35.433)
          (xy 4.5466 -34.925)
          (xy 4.2926 -34.925)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.064 -4.953)
          (xy 4.572 -4.445)
          (xy 4.318 -4.445)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.2926 -36.068)
          (xy 4.8006 -35.56)
          (xy 4.5466 -35.56)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 -5.588)
          (xy 4.826 -5.08)
          (xy 4.572 -5.08)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.7846 -36.322)
          (xy 1.8796 -36.322)
          (xy 2.8956 -34.798)
          (xy 3.7846 -36.322)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -36.322)
          (xy 1.905 -36.322)
          (xy 2.921 -34.798)
          (xy 3.81 -36.322)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -5.842)
          (xy 1.905 -5.842)
          (xy 2.921 -4.318)
          (xy 3.81 -5.842)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 35.8775 -9.4615)
          (xy 35.8775 -20.8915)
          (xy 28.1305 -20.8915)
          (xy 28.1305 -18.3515)
          (xy 26.8605 -18.3515)
          (xy 26.8605 -17.0815)
          (xy 25.5905 -17.0815)
          (xy 25.5905 -13.2715)
          (xy 26.8605 -13.2715)
          (xy 26.8605 -12.0015)
          (xy 28.1305 -12.0015)
          (xy 28.1305 -9.4615)
          (xy 35.8775 -9.4615)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7337 -17.78) (mid 7.366 -17.145) (end 6.7337 -16.51)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7364 -21.59) (mid 7.3687 -20.955) (end 6.7364 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7364 -20.32) (mid 7.3687 -19.685) (end 6.7364 -19.05)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7364 -19.05) (mid 7.3687 -18.415) (end 6.7364 -17.78)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7364 -10.16) (mid 7.3687 -9.525) (end 6.7364 -8.89)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7391 -13.97) (mid 7.3714 -13.335) (end 6.7391 -12.7)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7391 -12.7) (mid 7.3714 -12.065) (end 6.7391 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 6.7391 -11.43) (mid 7.3714 -10.795) (end 6.7391 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8846 -19.05) (mid 8.2523 -19.685) (end 8.8846 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8846 -17.78) (mid 8.2523 -18.415) (end 8.8846 -19.05)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8846 -16.51) (mid 8.2523 -17.145) (end 8.8846 -17.78)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8846 -11.43) (mid 8.2523 -12.065) (end 8.8846 -12.7)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8846 -10.16) (mid 8.2523 -10.795) (end 8.8846 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8846 -8.89) (mid 8.2523 -9.525) (end 8.8846 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8873 -20.32) (mid 8.255 -20.955) (end 8.8873 -21.59)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 8.8873 -12.7) (mid 8.255 -13.335) (end 8.8873 -13.97)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 10.16 -9.5277) (mid 10.795 -10.16) (end 11.43 -9.5277)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 10.2235 -17.2112) (mid 10.8585 -17.8435) (end 11.4935 -17.2112)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 11.43 -20.8253) (mid 10.795 -20.193) (end 10.16 -20.8253)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 11.43 -13.2053) (mid 10.795 -12.573) (end 10.16 -13.2053)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 11.43 -9.525) (mid 12.065 -10.1573) (end 12.7 -9.525)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 11.4935 -17.2085) (mid 12.1285 -17.8408) (end 12.7635 -17.2085)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 12.7 -20.8226) (mid 12.065 -20.1903) (end 11.43 -20.8226)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 12.7 -13.2026) (mid 12.065 -12.5703) (end 11.43 -13.2026)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (rectangle (start 16.002 -38.354) (end 17.272 -35.56)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (rectangle (start 17.78 -38.354) (end 19.05 -35.56)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (text "75" (at 16.637 -36.957 900)
        (effects (font (size 0.635 0.635)))
      )
      (text "75" (at 18.415 -36.957 900)
        (effects (font (size 0.635 0.635)))
      )
      (text "Green" (at 5.08 -35.56 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (text "LED_L" (at 3.81 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "LED_R" (at 3.81 -38.1 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Shield" (at 13.3858 -39.5986 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Shield" (at 22.0218 -39.5986 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Yellow" (at 5.08 -5.08 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (pin power_out line (at -2.54 -31.75 0) (length 2.54)
        (name "VC2-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -8.89 0) (length 2.54)
        (name "TD+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -36.83 0) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -34.29 0) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -6.35 0) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -3.81 0) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.78 -43.18 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 21.59 -43.18 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -26.67 0) (length 2.54)
        (name "VC1-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -21.59 0) (length 2.54)
        (name "RD-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -19.05 0) (length 2.54)
        (name "RCT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -16.51 0) (length 2.54)
        (name "RD+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -29.21 0) (length 2.54)
        (name "VC2+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -24.13 0) (length 2.54)
        (name "VC1+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 22.86 -13.97 180) (length 0) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -13.97 0) (length 2.54)
        (name "TD-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -11.43 0) (length 2.54)
        (name "TCT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RS8552" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RS8552" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2010160333_Jiangsu-RUNIC-Tech-RS8554XP_C236997.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "dual opamp" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Operational Amplifiers, DIP-8/SOIC-8/TSSOP-8/VSSOP-8" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RS8552_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "RS8552_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "RS8552_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "R_Y169010R0000T9L" (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "10" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220F-4_Horizontal_TabDown" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.hk/datasheet/2/428/vpr22021-3247675.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "Y169010R0000T9L" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Precision Power Resistor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "VPR221 and VPR221Z Series Precision Power Resistor, " (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "R_Y169010R0000T9L_0_1"
      (rectangle (start -1.016 2.54) (end 1.016 -2.54)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -3.81)
          (xy 0 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 3.81)
          (xy 0 3.81)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "R_Y169010R0000T9L_1_1"
      (pin passive line (at 0 5.08 270) (length 1.27)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 3.81 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -3.81 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 90) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SPDT_204-121ST" (in_bom yes) (on_board yes)
    (property "Reference" "SW" (at 1.27 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:204-121ST" (at 3.81 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ctscorp.com/wp-content/uploads/204.pdf" (at 5.08 -7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "204-121ST" (at 5.08 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SPDT_204-121ST_0_0"
      (polyline
        (pts
          (xy 3.556 -5.334)
          (xy 6.35 -6.35)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.556 -0.254)
          (xy 7.112 -0.6604)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -5.08)
          (xy 5.08 -5.715)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -3.81)
          (xy 5.08 -4.445)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -2.54)
          (xy 5.08 -3.175)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -1.27)
          (xy 5.08 -1.905)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 3.048 -5.08) (radius 0.508)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 3.048 0) (radius 0.508)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 7.112 -5.08) (radius 0.508)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 7.112 0) (radius 0.508)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "SPDT_204-121ST_1_1"
      (pin passive line (at 0 0 0) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -5.08 180) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "STM809SWX6F" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "STM809SWX6F" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at -7.62 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -7.62 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM809SWX6F_0_0"
      (pin power_in line (at -7.62 -2.54 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 2.54 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM809SWX6F_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "Screw" (in_bom yes) (on_board no)
    (property "Reference" "SCREW" (at 3.048 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "" (at 0 -2.413 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -1.27 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -1.27 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Screw_0_1"
      (polyline
        (pts
          (xy -0.254 0)
          (xy -0.635 -0.381)
          (xy -0.381 -0.635)
          (xy 0 -0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -0.254)
          (xy 0.381 -0.635)
          (xy 0.635 -0.381)
          (xy 0.254 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 0.254)
          (xy -0.381 0.635)
          (xy -0.635 0.381)
          (xy -0.254 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.254 0)
          (xy 0.635 0.381)
          (xy 0.381 0.635)
          (xy 0 0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 0 0) (radius 1.524)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
  )
  (symbol "TLV2172" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TLV2172IDGKT" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Footprint" "Package_SO:VSSOP-8_3.0x3.0mm_P0.65mm" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv172.pdf?ts=1697182483141&ref_url=https%253A%252F%252Fwww.google.com%252F" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "TLV2172IDGKT" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "TLV2172_1_1"
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 12.7 -2.54)
          (xy 2.54 -7.62)
          (xy 2.54 2.54)
          (xy 2.54 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 15.24 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 5.08 -8.89 90) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 5.08 3.81 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TLV2172_2_1"
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 12.7 -2.54)
          (xy 2.54 -7.62)
          (xy 2.54 2.54)
          (xy 2.54 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at 0 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS54620" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS54620" (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:Texas_S-PVQFN-N14" (at -7.62 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -7.62 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS54620_0_0"
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "RT/CLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 2.54 180) (length 2.54)
        (name "PH" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "PH" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 10.16 180) (length 2.54)
        (name "BOOT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -2.54 0) (length 2.54)
        (name "PWRGD" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -10.16 0) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 10.16 0) (length 2.54)
        (name "PVIN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 7.62 0) (length 2.54)
        (name "PVIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -5.08 180) (length 2.54)
        (name "VSENSE" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -7.62 180) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -10.16 180) (length 2.54)
        (name "SS/TR" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TPS54620_0_1"
      (rectangle (start -7.62 12.7) (end 7.62 -12.7)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
)
