(footprint "1156915" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -2.54 -13.97 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 4eed9204-1cf4-433a-b578-328643d1782a)
  )
  (fp_text value "1156915" (at 0 -7.62 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3290a7c7-cf39-4271-88f4-cf905e68497e)
  )
  (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp be5bb610-2469-4b6b-a6fa-231af202abe6)
  )
  (fp_line (start -4.699 -12.954) (end -0.381 -12.954)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 7409ae34-af3c-4b67-b7ce-e97eddcdf239))
  (fp_rect (start -5.08 -12.7) (end 5.08 12.7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 2e0aeada-2ba3-40ec-9369-7ba060beddd3))
  (fp_line (start -3.6 -11.75) (end -3.6 -11.11)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd9a5a34-ae1e-4057-b88a-07bd83ae31d0))
  (fp_line (start -3.6 -11.11) (end -2.54 -11.11)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b84a92e-e4b6-43f2-b4a9-18936671b7a0))
  (fp_line (start -3.6 -9.21) (end -3.6 -8.57)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5c0e394-5598-4239-9c9a-7ea3c5362b8b))
  (fp_line (start -3.6 -8.57) (end -2.54 -8.57)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 54332479-02b8-4e63-8862-8a7331b4eaf6))
  (fp_line (start -3.6 -6.67) (end -3.6 -6.03)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9495ce5-696b-4335-ba58-6cdfb5c2b386))
  (fp_line (start -3.6 -6.03) (end -2.54 -6.03)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6fdb13d9-1664-4e95-a982-8bdc06c010a6))
  (fp_line (start -3.6 -4.13) (end -3.6 -3.49)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea41e5fb-5789-41c6-8a03-af59ae50f9dc))
  (fp_line (start -3.6 -3.49) (end -2.54 -3.49)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a64d58b3-afbd-4731-afe2-c5fee8046233))
  (fp_line (start -3.6 -1.59) (end -3.6 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a7f6ce22-783c-40c4-8d4c-c1130a0da23e))
  (fp_line (start -3.6 -0.95) (end -2.54 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f6472787-8f59-4694-a9d4-43b73c2a461a))
  (fp_line (start -3.6 0.884) (end -3.6 1.524)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a94e18b6-e566-4e59-83e8-17147ea3a063))
  (fp_line (start -3.6 1.524) (end -2.54 1.524)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38bbff8e-9eed-420a-a39b-c7105c625008))
  (fp_line (start -3.6 3.424) (end -3.6 4.064)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4fc40cfd-5823-4a26-b501-eab9fcbc6d8d))
  (fp_line (start -3.6 4.064) (end -2.54 4.064)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 154db1e1-4568-43d3-a380-02c1d5136e4e))
  (fp_line (start -3.6 5.964) (end -3.6 6.604)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19d49163-9053-41cb-8b20-0c78182cf4ea))
  (fp_line (start -3.6 6.604) (end -2.54 6.604)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5073fdc6-f6ef-451e-8f3d-74e2b461ec8a))
  (fp_line (start -3.6 8.504) (end -3.6 9.144)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 47ae5c56-a2f9-4852-afe7-cc38bd75f166))
  (fp_line (start -3.6 9.144) (end -2.54 9.144)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50805166-8b74-40de-975c-bea6241a747f))
  (fp_line (start -3.6 11.044) (end -3.6 11.684)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8835393c-f62c-498d-af3c-ff9329c36dac))
  (fp_line (start -3.6 11.684) (end -2.54 11.684)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e834cd88-3e30-4ec9-af86-6b1c8baeb1d5))
  (fp_line (start -2.54 -11.75) (end -3.6 -11.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp acfcef7e-22a9-4d21-a111-b4394a6cdf6f))
  (fp_line (start -2.54 -11.75) (end -1.59 -12.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4a42fbfa-4212-4ad8-b87a-c4a8b3abf20e))
  (fp_line (start -2.54 -9.21) (end -3.6 -9.21)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9dc37fd8-998f-4029-b055-59053a887adf))
  (fp_line (start -2.54 -6.67) (end -3.6 -6.67)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 61c093b4-2020-4fba-a311-8b25e11cb315))
  (fp_line (start -2.54 -4.13) (end -3.6 -4.13)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce9f31a7-07e9-44c6-b1ca-9da09757deb4))
  (fp_line (start -2.54 -1.59) (end -3.6 -1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ffffcad-00ee-4e53-bab3-a72ddf6a72bc))
  (fp_line (start -2.54 0.63) (end -2.54 -11.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 357efed1-b309-4be7-82df-40c0257a6504))
  (fp_line (start -2.54 0.884) (end -3.6 0.884)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa2ca273-e414-4a90-bbd0-27c77547cca5))
  (fp_line (start -2.54 3.424) (end -3.6 3.424)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7facf333-a91a-47e6-b1a2-23512cfe6ba0))
  (fp_line (start -2.54 5.964) (end -3.6 5.964)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 530e5aaa-cf86-4c34-9128-a4b7893fcbdd))
  (fp_line (start -2.54 8.504) (end -3.6 8.504)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 619e485d-d2fa-410c-910e-edf6834d0b8a))
  (fp_line (start -2.54 11.044) (end -3.6 11.044)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60e2f208-2c0c-4bff-9e88-c4a4fa936c77))
  (fp_line (start -2.54 12.634) (end -2.54 0.884)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1574a631-c4a6-48ff-ae96-5716013c5f64))
  (fp_line (start -1.59 -12.7) (end 2.54 -12.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7833d4a-1ecd-4591-bd5a-62247430c7e5))
  (fp_line (start 2.54 -12.7) (end 2.54 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 068ba363-5246-48ee-8093-8122b4ace36f))
  (fp_line (start 2.54 -11.75) (end 3.6 -11.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dd78e1ed-ca6c-4417-b95a-2df9067839bb))
  (fp_line (start 2.54 -9.21) (end 3.6 -9.21)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 251404dc-442d-47fa-9224-26a6d834dd96))
  (fp_line (start 2.54 -6.67) (end 3.6 -6.67)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9e47ff68-9639-4c6d-9b1f-cd3daf05762e))
  (fp_line (start 2.54 -4.13) (end 3.6 -4.13)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a1c6d6d9-c380-4cc6-aa02-53aa60f655d5))
  (fp_line (start 2.54 -1.59) (end 3.6 -1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 864c7dd7-d04b-4369-bb1a-bb1cc94e47ba))
  (fp_line (start 2.54 -0.452) (end 2.54 12.248)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 848bff90-679c-4f2a-a9a6-4e496bc38299))
  (fp_line (start 2.54 0.884) (end 3.6 0.884)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5dfd73c-b5ee-4023-bf94-88d67a17ab7b))
  (fp_line (start 2.54 3.424) (end 3.6 3.424)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b9cdf5a-ff2b-4548-8dbe-23171a6eeccc))
  (fp_line (start 2.54 5.964) (end 3.6 5.964)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 676dd768-4201-4cee-ac60-f655bf15777c))
  (fp_line (start 2.54 8.504) (end 3.6 8.504)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc70136f-6d80-41bd-844d-a0e11f3c4f97))
  (fp_line (start 2.54 11.044) (end 3.6 11.044)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3a777a60-08eb-4dd5-ad01-edcea49c3fdd))
  (fp_line (start 2.54 12.634) (end -2.54 12.634)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aaf09344-122e-4af8-bbd4-8a145e425b01))
  (fp_line (start 3.6 -11.75) (end 3.6 -11.11)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee5f780b-bce8-40f2-aefa-1be87b2aafea))
  (fp_line (start 3.6 -11.11) (end 2.54 -11.11)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 84ba8bf2-d8d5-4cc4-842e-fbe4744e8c0a))
  (fp_line (start 3.6 -9.21) (end 3.6 -8.57)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e93e0709-4e36-4aaf-8ebe-a6167d438057))
  (fp_line (start 3.6 -8.57) (end 2.54 -8.57)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d615e4f1-d7a4-411a-bc42-2b40581204d5))
  (fp_line (start 3.6 -6.67) (end 3.6 -6.03)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0e7cff40-2d60-4e06-8692-7a7fdda500fa))
  (fp_line (start 3.6 -6.03) (end 2.54 -6.03)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3114cd0c-9dee-4e8d-ba2c-e29e26a76ec1))
  (fp_line (start 3.6 -4.13) (end 3.6 -3.49)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c539903-816e-4e3f-aa07-13131619d11f))
  (fp_line (start 3.6 -3.49) (end 2.54 -3.49)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a4150518-6fc2-4b74-bc37-3a81b8c7512d))
  (fp_line (start 3.6 -1.59) (end 3.6 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cb272109-4321-40d9-8835-90870ac5c5c4))
  (fp_line (start 3.6 -0.95) (end 2.54 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48089434-ad15-414c-a7cd-93bc91519ede))
  (fp_line (start 3.6 0.884) (end 3.6 1.524)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0226b940-d64f-4e3b-b383-796510055d5a))
  (fp_line (start 3.6 1.524) (end 2.54 1.524)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 733f056a-c248-4d89-9a4f-2a1dd6201fa1))
  (fp_line (start 3.6 3.424) (end 3.6 4.064)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 862262be-cd20-4cbc-a114-fc715799bbb7))
  (fp_line (start 3.6 4.064) (end 2.54 4.064)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 281e0c47-6f38-44fd-b52d-82931e4e75bb))
  (fp_line (start 3.6 5.964) (end 3.6 6.604)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1fd4942a-e0ce-4370-b50a-8c16444728ba))
  (fp_line (start 3.6 6.604) (end 2.54 6.604)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 08893bc3-254e-4bb9-b7c7-d1b5dd960fd7))
  (fp_line (start 3.6 8.504) (end 3.6 9.144)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9963af4c-a26f-4bc1-b811-f240a3dea20b))
  (fp_line (start 3.6 9.144) (end 2.54 9.144)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 717a79d4-c3ba-4789-9987-6761a377b44f))
  (fp_line (start 3.6 11.044) (end 3.6 11.684)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65d63ffc-2570-4230-8b62-ff96d10968be))
  (fp_line (start 3.6 11.684) (end 2.54 11.684)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp abb00be1-6709-4b9e-a7b3-d9ab9228eab5))
  (pad "" np_thru_hole circle (at 0 -10.16 90) (size 1.78 1.78) (drill 1.78) (layers "F&B.Cu" "*.Mask") (tstamp efc2e9d6-c449-4642-a85a-6035ca84a233))
  (pad "" np_thru_hole circle (at 0 10.16 90) (size 1.78 1.78) (drill 1.78) (layers "F&B.Cu" "*.Mask") (tstamp 1afe0908-5d4e-41d2-96c1-8d2cf975d0d9))
  (pad "1" smd roundrect (at -2.7 -11.43 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e5bf85e5-e80e-405c-8031-d138b7f18c52))
  (pad "2" smd roundrect (at 2.7 -11.43 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e09e5b84-3a48-4056-b1ea-bda3b5264183))
  (pad "3" smd roundrect (at -2.7 -8.89 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 336c9459-2d80-49a3-b945-8d99f3860af3))
  (pad "4" smd roundrect (at 2.7 -8.89 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0bac8267-3e02-467b-ae9e-781f841da28e))
  (pad "5" smd roundrect (at -2.7 -6.35 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 6f563145-62c2-442e-a60b-4240c00387ac))
  (pad "6" smd roundrect (at 2.54 -6.35 90) (size 1.02 3.185) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7dee4a39-7813-40b5-8c5a-8fdce2113c27))
  (pad "7" smd roundrect (at -2.7 -3.81 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1212b716-793f-4948-82f5-5597c3757402))
  (pad "8" smd roundrect (at 2.7 -3.81 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 82cf0efb-2c5f-4c14-aaaf-7153e18bd971))
  (pad "9" smd roundrect (at -2.7 -1.27 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 4850a1aa-c259-4f27-8217-30220ac877b7))
  (pad "10" smd roundrect (at 2.7 -1.27 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 62938fae-0d14-479e-ab58-879d8877593c))
  (pad "11" smd roundrect (at -2.7 1.27 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp c7af0749-8f71-4e07-a16a-f1e7d0b912dd))
  (pad "12" smd roundrect (at 2.7 1.27 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f97cda43-749d-49ea-8107-14adf397c329))
  (pad "13" smd roundrect (at -2.7 3.81 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 81591e5f-5bbc-4863-b71b-63d6c7688207))
  (pad "14" smd roundrect (at 2.7 3.81 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2d7afb30-682c-476f-ad62-f1a3855be5bf))
  (pad "15" smd roundrect (at -2.7 6.35 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2fc12f70-5839-43c6-88e8-e3c660357426))
  (pad "16" smd roundrect (at 2.54 6.35 90) (size 1.02 3.185) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1d74cd3e-eb6c-4688-b29a-8787a8f6e09a))
  (pad "17" smd roundrect (at -2.7 8.89 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 25151d16-f3c9-4f69-b10d-3eb04490bfea))
  (pad "18" smd roundrect (at 2.7 8.89 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5ae6828b-e1ac-4b9f-99a7-84a30fe5cfd3))
  (pad "19" smd roundrect (at -2.7 11.43 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp cff9b830-ef80-47c8-95eb-03f135dca0d4))
  (pad "20" smd roundrect (at 2.7 11.43 90) (size 1.02 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 9d348328-5e17-4cd6-97d0-7931ddf828bd))
  (model "${KIPRJMOD}/kirdy.pretty/1156915_00_00_FQ-2-54D-20-PV-380-1-BT_3D.stp"
    (offset (xyz -2 12.4 1))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
