(footprint "PM1202" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 27.94 0 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5c90fee6-64a7-4748-b73d-fb880ce13cf1)
  )
  (fp_text value "PM1202" (at 1.4 -3.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4348725f-78f2-44b9-884d-46648379c99e)
  )
  (fp_text user "${REFERENCE}" (at 9.4 -3.8 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aeafd2d5-7ab5-4c2c-88e9-934994ab193e)
  )
  (fp_line (start -1.27 -7.3) (end -1.27 2.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp ca5515e5-3523-4407-9647-1b5bf038e4f1))
  (fp_line (start -1.27 -7.3) (end 60.859 -7.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp db35ad12-f3c2-4b03-b3af-be4724bcb3a4))
  (fp_line (start -1.27 2.3) (end -1.27 11.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp a4a64db0-3332-4613-9acd-a2615645f1f2))
  (fp_line (start -1.27 11.3) (end 60.859 11.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp 3f8d04eb-14b7-45cc-b91d-39643f918dbc))
  (fp_line (start 60.859 0) (end 60.859 -7.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp eb8751bc-dcef-475b-b0ce-bb2bb82080ee))
  (fp_line (start 60.859 0) (end 60.859 2.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp d9f661a8-5931-4a8d-a364-3712d92e39b5))
  (fp_line (start 60.859 11.3) (end 60.859 2.3)
    (stroke (width 0.05) (type solid)) (layer "F.SilkS") (tstamp b03d0023-6e95-4af0-9b2d-0638acfa4d71))
  (fp_line (start -1.27 -7.3) (end -1.27 2.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a878e5f4-5345-4e34-b881-422fbcd57f48))
  (fp_line (start -1.27 -7.3) (end 60.859 -7.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9f5d5a4d-3d22-44ef-bbfb-5bc191ab05c5))
  (fp_line (start -1.27 2.3) (end -1.27 11.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25b0aa80-baee-43a0-b506-7c917421cfce))
  (fp_line (start -1.27 11.3) (end 60.859 11.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 99fae3ed-3f7d-4a12-86da-00d83880beac))
  (fp_line (start 60.859 0) (end 60.859 -7.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c16d2b9a-1c39-4800-8c04-47ccda6c6d03))
  (fp_line (start 60.859 0) (end 60.859 2.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb70420b-90c7-4b5b-8323-ed4b18da56ab))
  (fp_line (start 60.859 11.3) (end 60.859 2.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4c0077bb-94a6-4281-a330-706c8cb25429))
  (pad "1" thru_hole roundrect (at 0 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp c77258b1-5265-4446-bd4f-bb39fc9fe986))
  (pad "2" thru_hole roundrect (at 2.54 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp ae3c1221-a098-49a1-8631-f067c74b1e08))
  (pad "3" thru_hole roundrect (at 5.08 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 13ca2e3f-659f-42d6-b273-7529532992c2))
  (pad "4" thru_hole roundrect (at 7.62 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 0dac0b26-cc05-4f21-89e2-2ea38003e73f))
  (pad "5" thru_hole roundrect (at 10.16 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 1b7e0f42-4467-4e80-8012-337024ae5fba))
  (pad "6" thru_hole roundrect (at 12.7 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 8e142d6a-c56f-4d47-ae5c-d64e5593baf6))
  (pad "7" thru_hole roundrect (at 52.202 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 9e7e18e1-302a-4340-812a-4b4f0207c545))
  (pad "8" thru_hole roundrect (at 54.742 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp f1ee8936-b66c-499a-bb0c-011645be4b90))
  (pad "9" thru_hole roundrect (at 57.282 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 21bc1437-5943-4214-b89d-8d1f5af94ac7))
  (pad "10" thru_hole roundrect (at 59.822 0) (size 1.8 3) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 153d6c8f-d83a-4010-9433-ae1675f36797))
  (model "${KIPRJMOD}/kirdy.pretty/PM1202.step"
    (offset (xyz 29.9 -2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
