(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "+18V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "#PWR" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value" "+18V" (at 0 3.556 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "power-flag" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power symbol creates a global label with name \"+18V\"" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "+18V_0_1"
      (polyline
        (pts
          (xy -0.762 1.27)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 0)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0.762 1.27)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "+18V_1_1"
      (pin power_in line (at 0 0 90) (length 0) hide
        (name "+1V8" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "AD5680" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AD5680" (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (at -8.89 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad5680.pdf" (at -8.89 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD5680_0_0"
      (pin power_in line (at 8.89 12.7 180) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 12.7 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 7.62 180) (length 2.54)
        (name "VFB" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 10.16 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 7.62 0) (length 2.54)
        (name "~{SYNC}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 5.08 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 2.54 0) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 2.54 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AD5680_0_1"
      (rectangle (start -6.35 15.24) (end 6.35 0)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "AD7172-2" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 8.89 -22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AD7172-2" (at -6.35 -22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (at 2.54 -25.4 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad7172-2.pdf" (at 46.99 -46.99 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "24 bit precision ADC" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD7172-2_0_0"
      (pin input line (at -13.97 1.27 0) (length 2.54)
        (name "AIN4" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 21.59 180) (length 2.54)
        (name "XTAL2/CLKIO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 13.97 16.51 180) (length 2.54)
        (name "DOUT/~{RDY}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 13.97 180) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 11.43 180) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 8.89 180) (length 2.54)
        (name "~{CS}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 6.35 180) (length 2.54)
        (name "~{SYNC}/~{ERR}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -8.89 180) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -19.05 180) (length 2.54)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 13.97 -3.81 180) (length 2.54)
        (name "REGCAPD" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 1.27 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 21.59 0) (length 2.54)
        (name "REF-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 -1.27 180) (length 2.54)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 11.43 0) (length 2.54)
        (name "AIN0" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 8.89 0) (length 2.54)
        (name "AIN1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 6.35 0) (length 2.54)
        (name "AIN2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 3.81 0) (length 2.54)
        (name "AIN3" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 24.13 0) (length 2.54)
        (name "REF+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -13.97 19.05 0) (length 2.54)
        (name "REFOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -13.97 -3.81 0) (length 2.54)
        (name "REGCAPA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -19.05 0) (length 2.54)
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -8.89 0) (length 2.54)
        (name "AVDD1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -11.43 0) (length 2.54)
        (name "AVDD2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 24.13 180) (length 2.54)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AD7172-2_0_1"
      (rectangle (start -11.43 26.67) (end 11.43 -21.59)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "ADP150AUJZ-3.3" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ADP150AUJZ-3.3" (at -7.62 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adp150.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low noise LDO" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ADP150AUJZ-3.3_0_0"
      (pin power_in line (at 5.08 10.16 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 5.08 7.62 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 13.97 8.89 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 10.16 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ADP150AUJZ-3.3_0_1"
      (rectangle (start 7.62 12.7) (end 20.32 0)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start 20.32 3.81) (end 20.32 3.81)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
  )
  (symbol "AG5300" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.35 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AG5300" (at -2.54 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:AG5300" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://silvertel.com/images/datasheets/Ag5300-datasheet-smallest-30W-Power-Over-Ethernet-Plus-Module-PoEplusPD.pdf" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "PoE" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PoE Module, 12V, 30W" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AG5300_0_0"
      (pin power_in line (at -8.89 7.62 0) (length 2.54)
        (name "VIN+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -2.54 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 -2.54 0) (length 2.54)
        (name "VIN-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -8.89 2.54 0) (length 2.54)
        (name "AT-DET" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -0.635 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0.635 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 1.905 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 7.62 180) (length 2.54)
        (name "+VDC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 3.81 180) (length 2.54)
        (name "ADJ" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AG5300_0_1"
      (rectangle (start -6.35 10.16) (end 7.62 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "Filter_EMI_LL_1423" (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "FL" (at 0 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Filter_EMI_LL_1423" (at 0 -4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB" (at 0 1.016 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 1.016 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "EMI filter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "EMI 2-inductor filter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "L_* L_CommonMode*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Filter_EMI_LL_1423_0_1"
      (circle (center -3.048 -1.27) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type outline))
      )
      (circle (center -3.048 1.524) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type outline))
      )
      (arc (start -2.54 2.032) (mid -2.032 1.5262) (end -1.524 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -1.524 -2.032) (mid -2.032 -1.5262) (end -2.54 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -1.524 2.032) (mid -1.016 1.5262) (end -0.508 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -0.508 -2.032) (mid -1.016 -1.5262) (end -1.524 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start -0.508 2.032) (mid 0 1.5262) (end 0.508 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.032)
          (xy -2.54 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 0.508)
          (xy 2.54 0.508)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 2.032)
          (xy -2.54 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -2.032)
          (xy 2.54 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -0.508)
          (xy -2.54 -0.508)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 2.54 2.032)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 0.508 -2.032) (mid 0 -1.5262) (end -0.508 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 0.508 2.032) (mid 1.016 1.5262) (end 1.524 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 1.524 -2.032) (mid 1.016 -1.5262) (end 0.508 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 1.524 2.032) (mid 2.032 1.5262) (end 2.54 2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (arc (start 2.54 -2.032) (mid 2.032 -1.5262) (end 1.524 -2.032)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "Filter_EMI_LL_1423_1_1"
      (pin passive line (at -5.08 2.54 0) (length 2.54)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 2.54 180) (length 2.54)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -2.54 180) (length 2.54)
        (name "3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -2.54 0) (length 2.54)
        (name "4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LAN8742A" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LAN8742A" (at 0 -27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (at 0 -33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/8742a.pdf" (at 2.54 -35.56 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LAN8742A_0_0"
      (pin power_in line (at 10.16 -7.62 180) (length 2.54)
        (name "VDD2A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "RXER" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 0 0) (length 2.54)
        (name "CRS_DV" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
        (name "MDIO" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "MDC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 -15.24 0) (length 2.54)
        (name "nINT" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 2.54)
        (name "nRST" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 20.32 0) (length 2.54)
        (name "TXEN" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "TXD0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 15.24 0) (length 2.54)
        (name "TXD1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VDD1A" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "LED2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 17.78 180) (length 2.54)
        (name "TXN" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 20.32 180) (length 2.54)
        (name "TXP" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 12.7 180) (length 2.54)
        (name "RXN" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 15.24 180) (length 2.54)
        (name "RXP" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "RBIAS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -22.86 180) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "LED1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 2.54)
        (name "XTAL2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -22.86 0) (length 2.54)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -12.7 180) (length 2.54)
        (name "VDDCR" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 7.62 0) (length 2.54)
        (name "RXD1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 10.16 0) (length 2.54)
        (name "RXD0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -10.16 180) (length 2.54)
        (name "VDDIO" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LAN8742A_0_1"
      (rectangle (start -10.16 22.86) (end 7.62 -25.4)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "LT3081xDF" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LT3081xDF" (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 30.48 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 30.48 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LT3081xDF_0_0"
      (pin power_out line (at 10.16 2.54 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54) hide
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54) hide
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54) hide
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54) hide
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 0 180) (length 2.54)
        (name "ILIM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 0 0) (length 2.54)
        (name "SET" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -8.89 -2.54 0) (length 2.54)
        (name "IMON" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "TEMP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 2.54 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LT3081xDF_0_1"
      (rectangle (start -6.35 5.08) (end 7.62 -5.08)
        (stroke (width 0.1524) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "LTC3261" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LTC3261" (at 0 -13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3261fb.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC3261_0_0"
      (pin no_connect line (at 0 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 3.81 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 1.27 180) (length 2.54)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 -8.89 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 3.81 180) (length 2.54)
        (name "RT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -1.27 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 8.89 6.35 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -8.89 0) (length 2.54)
        (name "C-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -3.81 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -1.27 0) (length 2.54)
        (name "C+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 6.35 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LTC3261_0_1"
      (rectangle (start -5.08 8.89) (end 6.35 -11.43)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start 48.26 -19.05) (end 48.26 -19.05)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (rectangle (start 48.26 -19.05) (end 48.26 -19.05)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (rectangle (start 48.26 -19.05) (end 48.26 -19.05)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
  )
  (symbol "LTC6655" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LTC6655" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:LCC127P500X500X155-8N" (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc6655-6655ln.pdf" (at -1.27 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "reference" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision series voltage reference" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC6655_0_0"
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "~{SHDN}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 2.54 180) (length 2.54)
        (name "VOUT_S" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 5.08 180) (length 2.54)
        (name "VOUT_F" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -2.54 0) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LTC6655_0_1"
      (rectangle (start -7.62 7.62) (end 8.89 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "MAX1968xUI" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX1968xUI" (at 5.08 16.51 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm" (at 0 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1968-MAX1969.pdf" (at 0 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "thermoelectric cooler" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power Driver for Peltier TEC Modules, +-3A, HTSSOP-28" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX1968xUI_0_1"
      (rectangle (start -7.62 15.24) (end 7.62 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "MAX1968xUI_1_1"
      (pin power_in line (at 0 17.78 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -7.62 180) (length 2.54) hide
        (name "LX2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 17.78 270) (length 2.54) hide
        (name "PVDD2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "FREQ" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -12.7 0) (length 2.54)
        (name "ITEC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -5.08 180) (length 2.54)
        (name "OS2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 0 180) (length 2.54)
        (name "OS1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 2.54 180) (length 2.54)
        (name "CS" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "~{SHDN}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 17.78 270) (length 2.54)
        (name "PVDD1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 5.08 180) (length 2.54)
        (name "LX1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 17.78 270) (length 2.54) hide
        (name "PVDD1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54) hide
        (name "LX1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -17.78 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54) hide
        (name "LX1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -17.78 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -10.16 0) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "MAXIN" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "MAXIP" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "MAXV" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -17.78 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "CTLI" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 2.54 0) (length 2.54)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -17.78 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -7.62 180) (length 2.54)
        (name "LX2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -17.78 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -7.62 180) (length 2.54) hide
        (name "LX2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 17.78 270) (length 2.54)
        (name "PVDD2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "PM1202" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.35 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PM1202" (at -2.54 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "kirdy:PM1202" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -21.59 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "PoE" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PoE Module, 12V, 30W" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PM1202_0_0"
      (pin no_connect line (at -2.54 6.35 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 5.08 180) (length 2.54)
        (name "+VDC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -0.635 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 7.62 0) (length 2.54)
        (name "VIN+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 -2.54 0) (length 2.54)
        (name "VIN-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0.635 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 1.905 5.715 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -2.54 180) (length 2.54)
        (name "-VDC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 7.62 180) (length 2.54)
        (name "+VDC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "PM1202_0_1"
      (rectangle (start -6.35 10.16) (end 7.62 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "RS8552" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RS8552" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2010160333_Jiangsu-RUNIC-Tech-RS8554XP_C236997.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "dual opamp" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Operational Amplifiers, DIP-8/SOIC-8/TSSOP-8/VSSOP-8" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RS8552_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "RS8552_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "RS8552_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "STM809SWX6F" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "STM809SWX6F" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at -7.62 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -7.62 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM809SWX6F_0_0"
      (pin power_in line (at -7.62 -2.54 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 2.54 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM809SWX6F_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "TLV2172" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TLV2172IDGKT" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Footprint" "Package_SO:VSSOP-8_3.0x3.0mm_P0.65mm" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv172.pdf?ts=1697182483141&ref_url=https%253A%252F%252Fwww.google.com%252F" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "TLV2172IDGKT" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "TLV2172_1_1"
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 12.7 -2.54)
          (xy 2.54 -7.62)
          (xy 2.54 2.54)
          (xy 2.54 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 15.24 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 5.08 -8.89 90) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 5.08 3.81 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TLV2172_2_1"
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 12.7 -2.54)
          (xy 2.54 -7.62)
          (xy 2.54 2.54)
          (xy 2.54 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at 0 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS54620" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 -17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS54620" (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:Texas_S-PVQFN-N14" (at -7.62 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -7.62 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS54620_0_0"
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "RT/CLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 2.54 180) (length 2.54)
        (name "PH" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "PH" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 10.16 180) (length 2.54)
        (name "BOOT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -2.54 0) (length 2.54)
        (name "PWRGD" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -10.16 0) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 10.16 0) (length 2.54)
        (name "PVIN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 7.62 0) (length 2.54)
        (name "PVIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -5.08 180) (length 2.54)
        (name "VSENSE" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -7.62 180) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -10.16 180) (length 2.54)
        (name "SS/TR" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TPS54620_0_1"
      (rectangle (start -7.62 12.7) (end 7.62 -12.7)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
)
