(footprint "CAPC1810X65N" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "GRMJN65C1H104JE01D")
  (tags "Capacitor")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 82fac2c8-7c52-4455-af14-53152ac84b3e)
  )
  (fp_text value "CAPC1810X65N" (at 0 0) (layer "F.SilkS") hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp 76be2609-84d0-45c9-8e12-5300bfa4edcb)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp 1b67f5b4-c82d-468d-a89c-421577efb106)
  )
  (fp_line (start 0 -0.4) (end 0 0.4)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 4a3078fb-4ad0-4f74-9bbb-ba86d81ea27c))
  (fp_line (start -1.325 -0.72) (end 1.325 -0.72)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30ebf5c2-6a78-435a-afc0-a1249bdf63d4))
  (fp_line (start -1.325 0.72) (end -1.325 -0.72)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 71bb3fed-7cbd-4f23-84b4-13bd7df3c5e8))
  (fp_line (start 1.325 -0.72) (end 1.325 0.72)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e81a65e6-ea8a-4e87-a150-d77160f47e41))
  (fp_line (start 1.325 0.72) (end -1.325 0.72)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d02e7b95-2277-4896-aaf7-f4f7ce3873da))
  (fp_line (start -0.9 -0.5) (end 0.9 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 117a39cd-074e-491c-8778-184a694ca1bd))
  (fp_line (start -0.9 0.5) (end -0.9 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9a0a1e9-a459-43b9-9cf6-aa56b818f5db))
  (fp_line (start 0.9 -0.5) (end 0.9 0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b9bd443-0f0e-4da8-82c0-867b91c85183))
  (fp_line (start 0.9 0.5) (end -0.9 0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9ba24b91-5166-4cb3-96d0-e3a743305be8))
  (pad "1" smd rect (at -0.8 0) (size 0.75 1.14) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 37d2c938-cba3-4270-9377-7847f9965d8d))
  (pad "2" smd rect (at 0.8 0) (size 0.75 1.14) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f02f5bb7-3f56-462a-97d2-e7a3a88f52dc))
  (model "GRMJN65C1H104JE01J.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
