(footprint "204-121ST" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0.635 -5.715 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 0531f170-e9ac-4ae6-a5e8-0799b9b181e8)
  )
  (fp_text value "204-121ST" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 56122884-337f-4a1b-a83b-35093594f0d8)
  )
  (fp_text user "ON" (at 3.175 -5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
    (tstamp 558dd1fc-41e7-4f6f-b890-9f992e5d4be6)
  )
  (fp_text user "OFF" (at -5.08 -5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
    (tstamp 6630a108-13aa-4074-806c-45611146dffb)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f4ad8b00-5dd6-49f2-b53e-1f2c9d8eebfc)
  )
  (fp_rect (start -6.5 -5) (end 6.5 5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 424a6d99-2b4a-42a2-9d74-af4915ab0bf2))
  (fp_rect (start -2.54 -2.54) (end 2.54 2.54)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 30997e09-7456-4ea5-97ae-3664699517e2))
  (fp_rect (start -1.905 -1.27) (end -0.635 1.27)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e6f98df9-5b7c-459d-ae92-c7e01b15121f))
  (fp_circle (center -5.08 3.81) (end -4.68 3.81)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 96a3e9fe-07d5-44fd-a112-0c41be2616bc))
  (fp_circle (center 5.08 -3.81) (end 5.48 -3.81)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 38f597a5-4f6e-4cff-b880-925f9c8312dc))
  (fp_rect (start -6.5 -5) (end 6.5 5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.CrtYd") (tstamp 8e512a23-705a-4504-8a3a-56e4c63f9f6e))
  (pad "1" smd roundrect (at -4.3 -1.27 90) (size 1.13 2.435) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d2837f54-3542-4f56-b73f-a2306014dc40))
  (pad "2" smd roundrect (at -4.3 1.27 90) (size 1.13 2.435) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 25258d7d-0f5c-482d-86fd-73fbe601894e))
  (pad "3" smd roundrect (at 4.3 1.27 90) (size 1.13 2.435) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 15eaa29d-b053-4428-a6c8-2b342ec834ba))
  (pad "4" smd roundrect (at 4.3 -1.27 90) (size 1.13 2.435) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 42125979-11e4-41d7-9e16-71a4b81a66e5))
  (model "${KIPRJMOD}/kirdy.pretty/204-121ST.stpz"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
