(footprint "SOIC8-TL082Hx" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -1.55 -3.4 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp f894710c-6e74-4c0f-9b0e-552a62c60455)
  )
  (fp_text value "SOIC8-TL082Hx" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6cc2d9f3-cb53-4a25-bcd5-fec828992fbf)
  )
  (fp_text user "${REFERENCE}" (at 0 2.46 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c3973aca-4d93-4a25-be58-f1af5729a1b2)
  )
  (fp_text user "${REFERENCE}" (at 0.2 -0.04) (layer "F.Fab")
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    (tstamp fb258ada-39e2-4eaf-a89b-525f2984123d)
  )
  (fp_line (start 0 -2.56) (end -3.45 -2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65561bb2-46b3-4864-b22c-a64612d61753))
  (fp_line (start 0 -2.56) (end 1.95 -2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 16da7bbf-57d3-4aff-97c1-3abd79137f25))
  (fp_line (start 0 2.56) (end -1.95 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2bbcc4a8-3478-4dc2-b23c-8de87839ceeb))
  (fp_line (start 0 2.56) (end 1.95 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c4d9089f-6bb0-4c07-9f95-f606f8f21631))
  (fp_line (start -3.825 -2.7) (end -3.825 2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3119a8e6-9fe6-4e10-b282-cf0ee9e7d2a5))
  (fp_line (start -3.825 2.7) (end 3.825 2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 91303c4d-6a4f-4317-a53c-69f9b5628519))
  (fp_line (start 3.825 -2.7) (end -3.825 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3e683e99-612d-47ef-9d0a-02740de9fd31))
  (fp_line (start 3.825 2.7) (end 3.825 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 845108d0-36fd-4346-9e24-cb49bfab80ab))
  (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49f59489-865b-4f45-acdc-a8f1b7ad0a73))
  (fp_line (start -1.95 2.45) (end -1.95 -1.475)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fe7fd8f4-b56d-4cb7-be70-2eb3ba46b258))
  (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e8fe4797-7c1f-4bdb-8c54-51bd50e24946))
  (fp_line (start 1.95 -2.45) (end 1.95 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cfb6fb2e-7999-4022-bd41-18ed25a98763))
  (fp_line (start 1.95 2.45) (end -1.95 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 831f5337-7066-4099-ae5d-e8555cbd9da1))
  (pad "1" smd roundrect (at -2.7 -1.905) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9d5fda7c-e9e7-4aca-bc62-b083951e2020))
  (pad "2" smd roundrect (at -2.7 -0.635) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ebda9735-f943-495a-80ad-792e6bca64ac))
  (pad "3" smd roundrect (at -2.7 0.635) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7620cec9-ae4f-457b-8a19-f9043aa2fc84))
  (pad "4" smd roundrect (at -2.7 1.905) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2cb3f8c7-9db3-4717-a814-764cb3db6dd1))
  (pad "5" smd roundrect (at 2.7 1.905) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2edc7a31-e8f3-4099-be58-808a204315d4))
  (pad "6" smd roundrect (at 2.7 0.635) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c9385aab-5dbe-4c78-b040-ba82257bb9e0))
  (pad "7" smd roundrect (at 2.7 -0.635) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5e688934-e374-438f-9d63-2a58eddcbbed))
  (pad "8" smd roundrect (at 2.7 -1.905) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f24a6370-2fc4-46e4-9995-18fcdade5153))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
