(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "butterfly_socket_type_1" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Butterfly_Socket" (at 7.62 -22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "laserSocket:Butterfly_Socket" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://m.tb.cn/h.5QDXYK1?tk=wr4mW3e8DlQ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "https://m.tb.cn/h.5QDXYK1?tk=wr4mW3e8DlQ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN_ALT" "Open on Mobile Version of Taobao. Communuicate with the vendor for customized part." (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "butterfly_socket_type_1_1_1"
      (rectangle (start 0 0) (end 20.32 -19.05)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start 6.35 -3.81) (end 13.97 -15.24)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (text "*: Alternate LD/PD Connections" (at 15.24 -20.32 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Type-1 LD" (at 10.16 -9.525 900)
        (effects (font (size 1.27 1.27)))
      )
      (pin input line (at -2.54 -2.54 0) (length 2.54)
        (name "TEC+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -12.7 180) (length 2.54)
        (name "LD+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -10.16 180) (length 2.54)
        (name "LD-" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 22.86 -7.62 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -5.08 180) (length 2.54)
        (name "Case" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -2.54 180) (length 2.54)
        (name "TEC-" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -5.08 0) (length 2.54)
        (name "NTC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -7.62 0) (length 2.54)
        (name "PD+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -10.16 0) (length 2.54)
        (name "PD-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -12.7 0) (length 2.54)
        (name "NTC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -15.24 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -17.78 0) (length 2.54)
        (name "PD-*" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -17.78 180) (length 2.54)
        (name "PD+*" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -15.24 180) (length 2.54)
        (name "LD-*" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "butterfly_socket_type_2" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Butterfly_Socket" (at 7.62 -20.32 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "laserSocket:Butterfly_Socket" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://m.tb.cn/h.5QDXYK1?tk=wr4mW3e8DlQ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "https://m.tb.cn/h.5QDXYK1?tk=wr4mW3e8DlQ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN_ALT" "Open on Mobile Version of Taobao. Communuicate with the vendor for customized part." (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "butterfly_socket_type_2_1_1"
      (rectangle (start 0 0) (end 22.86 -19.05)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start 7.62 -3.81) (end 15.24 -15.24)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (text "Type-2 LD" (at 11.43 -9.525 900)
        (effects (font (size 1.27 1.27)))
      )
      (pin input line (at -2.54 -2.54 0) (length 2.54)
        (name "NTC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 25.4 -12.7 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.4 -10.16 180) (length 2.54)
        (name "LD+" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.4 -7.62 180) (length 2.54)
        (name "Mod_In" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.4 -5.08 180) (length 2.54)
        (name "LD+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 25.4 -2.54 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -5.08 0) (length 2.54)
        (name "NTC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -7.62 0) (length 2.54)
        (name "LD-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -10.16 0) (length 2.54)
        (name "PD+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -12.7 0) (length 2.54)
        (name "PD-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -15.24 0) (length 2.54)
        (name "TEC+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -17.78 0) (length 2.54)
        (name "TEC-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.4 -17.78 180) (length 2.54)
        (name "Case" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.4 -15.24 180) (length 2.54)
        (name "Case" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "kirdy_3d_model" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "kirdy" (at 3.81 -1.905 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "laserSocket:kirdy_socket" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "kirdy" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "kirdy_3d_model_1_1"
      (rectangle (start 0 0) (end 7.62 -3.81)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "kirdy_socket_1" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "M20-7870542" (at 10.16 -12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "laserSocket:M20-7870542" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "M20-7870542" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "kirdy_socket_1_1_1"
      (rectangle (start 3.81 -10.033) (end 4.445 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 4.445 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 4.445 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 4.445 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 4.445 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 1.27) (end 16.51 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 15.875 -10.033) (end 16.51 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -7.493) (end 16.51 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -4.953) (end 16.51 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -2.413) (end 16.51 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 0.127) (end 16.51 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at 0 0 0) (length 3.81)
        (name "NTC-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -10.16 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 0 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 0) (length 3.81)
        (name "NTC+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -2.54 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -5.08 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 0) (length 3.81)
        (name "TEC-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -7.62 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -10.16 0) (length 3.81)
        (name "TEC+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "kirdy_socket_2" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "M20-7870542" (at 10.16 -12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "laserSocket:M20-7870542" (at -1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MFR_PN" "M20-7870542" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "kirdy_socket_2_1_1"
      (rectangle (start 3.81 -10.033) (end 4.445 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 4.445 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 4.445 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 4.445 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 4.445 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 1.27) (end 16.51 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 15.875 -10.033) (end 16.51 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -7.493) (end 16.51 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -4.953) (end 16.51 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 -2.413) (end 16.51 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 15.875 0.127) (end 16.51 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at 0 0 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -10.16 180) (length 3.81)
        (name "PD-" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 0 180) (length 3.81)
        (name "LD+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -2.54 180) (length 3.81)
        (name "LD-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -5.08 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -7.62 180) (length 3.81)
        (name "PD+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -10.16 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
