(module BOURNS-GDT-2051 (layer F.Cu) (tedit 553CF70D)
  (attr smd)
  (fp_text reference REF** (at 0 0) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value BOURNS-GDT-2051 (at 0 0) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -3 -2) (end 3 -2) (layer F.Fab) (width 0.2))
  (fp_line (start 3 -2) (end 3 2) (layer F.Fab) (width 0.2))
  (fp_line (start 3 2) (end -3 2) (layer F.Fab) (width 0.2))
  (fp_line (start -3 2) (end -3 -2) (layer F.Fab) (width 0.2))
  (fp_line (start 1 -1.5) (end 1 1.5) (layer F.SilkS) (width 0.2))
  (fp_line (start 1 1.5) (end 0 0) (layer F.SilkS) (width 0.2))
  (fp_line (start 0 0) (end 1 -1.5) (layer F.SilkS) (width 0.2))
  (fp_line (start -1 -1.5) (end -1 1.5) (layer F.SilkS) (width 0.2))
  (fp_line (start -1 1.5) (end 0 0) (layer F.SilkS) (width 0.2))
  (fp_line (start 0 0) (end -1 -1.5) (layer F.SilkS) (width 0.2))
  (fp_line (start -3.25 -2.35) (end 3.25 -2.35) (layer F.CrtYd) (width 0.2))
  (fp_line (start 3.25 -2.35) (end 3.25 2.35) (layer F.CrtYd) (width 0.2))
  (fp_line (start 3.25 2.35) (end -3.25 2.35) (layer F.CrtYd) (width 0.2))
  (fp_line (start -3.25 2.35) (end -3.25 -2.35) (layer F.CrtYd) (width 0.2))
  (pad 1 smd rect (at -2.25 0) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.25 0) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask))
)