(module Connectors_Phoenix:PhoenixContact_MC-G_03x5.08mm_Angled (layer F.Cu) (tedit 58F9A094)
  (descr PhoenixContact_1786417_03x5.08mm_Angled)
  (tags "phoenix_contact connector 01x03_G_5.08mm")
  (fp_text reference REF** (at 4.826 -4.064) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PhoenixContact_1786417_03x5.08mm_Angled (at 5.08 9.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.62 -3) (end -2.62 16) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.62 16) (end 12.78 16) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.78 16) (end 12.78 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.62 -3) (end 12.78 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.62 8) (end 12.78 8) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -2.3) (end 0.3 -2.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.3 -2.9) (end -0.3 -2.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.3 -2.9) (end 0 -2.3) (layer F.SilkS) (width 0.15))
  (pad 3 thru_hole oval (at 10.16 5.08) (size 2.5 3.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 5.08 5.08) (size 2.5 3.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 5.08) (size 2.5 3.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 2.5 3.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 5.08 0) (size 2.5 3.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 10.16 0) (size 2.5 3.6) (drill 1.6) (layers *.Cu *.Mask))
)
