(module proj_footprints:BOURNS-GDT-2035TH (layer F.Cu) (tedit 598482D8)
  (descr "relay, Coto 9001 series Reed")
  (fp_text reference GDT*** (at 0 -4.1) (layer F.SilkS)
    (effects (font (thickness 0.3048)))
  )
  (fp_text value 2035 (at 0 4.3) (layer F.SilkS) hide
    (effects (font (thickness 0.3048)))
  )
  (fp_line (start -3 -3) (end 3 -3) (layer F.SilkS) (width 0.3048))
  (fp_line (start 3 -3) (end 3 3) (layer F.SilkS) (width 0.3048))
  (fp_line (start -3 3) (end 3 3) (layer F.SilkS) (width 0.3048))
  (fp_line (start -3 3) (end -3 -3) (layer F.SilkS) (width 0.3048))
  (pad 1 thru_hole circle (at -3.81 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 3.81 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
)
