\input{preamble.tex}
\graphicspath{{images/1106}, {images}}

\title{1106 EEM AC Power Module}
\author{M-Labs Limited}
\date{January 2025}
\revision{Revision 1}
\companylogo{\includegraphics[height=0.73in]{artiq_sinara.pdf}}

\begin{document}
\maketitle

\section{Features}

    \begin{itemize}
        \item{Front panel IEC inlet}
        \item{80-264V input range}
        \item{Five 4-pin Molex MiniFit outputs}
        \item{EMC filter}
    \end{itemize}

\section{Applications}

    \begin{itemize}
        \item{Power supply for ARTIQ/Sinara systems}
        \item{Provides 400W at 25CFM cooling, 200W with free air convection}
    \end{itemize}

\section{General Description}

    The 1106 EEM AC Power Module is a 8hp EEM form factor module, part of the ARTIQ/Sinara family. It serves as an in-crate power supply to other Sinara cards such as 1124 Carrier Kasli 2.0 and 1125 Carrier Kasli-SoC.

    The AC Power Module features universal IEC input in the front panel and five 4-pin Molex output, directly compatible with Kasli Carriers, at the very rear side of the module. The mains circuit is protected by a steel cover.

% Switch to next column
\vfill\break

%\begin{figure}[h]
%    \centering
%    \scalebox{1.15}{
%    \begin{circuitikz}[european, every label/.append style={align=center}]
%        \begin{scope}[]
%            % if applicable
%        \end{scope}
%    \end{circuitikz}
%    }

%    \caption{Simplified Block Diagram}
%\end{figure}

\begin{figure}[hbt!]
    \centering
    \includegraphics[height=2.5in]{photo1106.jpg}
    \caption{EEM AC Power Module with handle}
    \includegraphics[height=2.5in, angle=90]{fp1106.pdf}
    \caption{EEM AC Power Module front panel}
\end{figure}

% For wide tables, a single column layout is better. It can be switched
% page-by-page.
\onecolumn

\sourcesection{1106 EEM AC Power Module}{https://github.com/sinara-hw/EEM_PWR_MOD_AC}

\section{Electrical Specifications}

Specifications of parameters are based on the datasheet of the EPP-400-12 power supply\footnote{\url{https://www.meanwell.com/upload/pdf/EPP-400/EPP-400-SPEC.PDF}}.

\begin{table}[h]
\centering
\begin{threeparttable}
\caption{Electrical Specifications}
\begin{tabularx}{0.75\textwidth}{l | c c c | c | X}
    \thickhline
    \textbf{Parameter} & \textbf{Min} & \textbf{Typ.} & \textbf{Max} & \textbf{Unit} & \textbf{Conditions} \\
    \hline
    Output voltage & & 12 & & V & \\ \hline
    \multirow{2}{*}{Rated current} & & 33.3 & & \multirow{2}{*}{A} & 25CFM forced cooling \\ \cline{2-4}
        & & 20.8 & & & Convection \\ \hline
    \multirow{2}{*}{Rated power} & & 399.6 & & \multirow{2}{*}{W} & 25CFM forced cooling \\ \cline{2-4}
        & & 249.6 & & & Convection \\ \hline
    Input voltage           & 80 & & 264    & VAC & \\ \hline
    Input frequency range   & 47 & & 63     & Hz  & \\ \hline
    \thickhline
\end{tabularx}
\end{threeparttable}
\end{table}

\section{Indicator LEDs}

The 1106 EEM AC Power Module features several indicator LEDs. Four serve as current indicators signaling 25\%, 50\%, 75\% and 100\% load. \texttt{12V} LED signals power on. Additional \texttt{OVERTEMP} LED signals overtemp or overload.

\ordersection{1106 EEM AC Power Module}

\finalfootnote

\end{document}
