(footprint "78614110360_Receptacle" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Small Receptacle Footprint for 78614110360")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -4.25 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 9a489406-4ef8-4b76-86fa-bad77d0d3ec6)
  )
  (fp_text value "78614110360" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 88c52b20-06ab-4987-ba5b-c34280174f26)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0e2863ec-f59a-4c98-9232-c7104e422184)
  )
  (fp_circle (center 0 0) (end 3.2 0)
    (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp cba62500-5259-4a17-b491-f4c0c32c1b8d))
  (fp_circle (center 0 0) (end 3.45 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 84c3fb36-0185-49d4-ade4-764684c6e995))
  (pad "1" thru_hole circle (at -2.2 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp d6e6880b-b3c4-44be-bb42-e60c610ea646))
  (pad "1" thru_hole circle (at -1.6 -1.6) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp e1dc9b4b-c997-4a29-a0b3-f5db0fd9ee85))
  (pad "1" thru_hole circle (at -1.6 1.6) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp ab57c4a0-7950-4295-9a52-f4f967dee60e))
  (pad "1" thru_hole circle (at 0 -2.2) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp cb5f495f-d0cf-4875-8128-a63eda929f8a))
  (pad "1" thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp 5be7e35b-77ad-449a-8913-42f00a6235d6))
  (pad "1" thru_hole circle (at 0 2.2) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp 70675791-59a8-4962-9a90-8967d71d0a19))
  (pad "1" thru_hole circle (at 1.6 -1.6) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp 177008f7-bfdd-455a-82e4-99b92d1424dc))
  (pad "1" thru_hole circle (at 1.6 1.6) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp 746d013e-b642-48f1-b55e-022854e0cbf2))
  (pad "1" thru_hole circle (at 2.2 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp bfb1ef03-4b50-49d2-9629-c34ba5ce034c))
)
