.. Always keep doc/manual/introduction.rst synchronized with this file, with the exception of the logo.

.. image:: doc/logo/artiq.png

ARTIQ (Advanced Real-Time Infrastructure for Quantum physics) is the next-generation control system for quantum information experiments.
It is developed by `M-Labs <https://m-labs.hk>`_ for and in partnership with the `Ion Storage Group at NIST <http://www.nist.gov/pml/div688/grp10/index.cfm>`_ as free software.
It is offered to the entire research community as a solution equally applicable to other challenging control tasks outside the field of ion trapping.

The system features a high-level programming language that helps describing complex experiments, which is compiled and executed on dedicated hardware with nanosecond timing resolution and sub-microsecond latency. It includes graphical user interfaces to parametrize and schedule experiments and to visualize and explore the results.

ARTIQ uses FPGA hardware to perform its time-critical tasks.
It is designed to be portable to hardware platforms from different vendors and FPGA manufacturers.
Currently, one configuration of a `low-cost open hardware FPGA board <http://pipistrello.saanlima.com/>`_ and several different configurations of a `high-end FPGA evaluation kit <http://www.xilinx.com/products/boards-and-kits/ek-k7-kc705-g.html>`_ are used and supported.
Any of these FPGA platforms can be combined with any number of additional peripherals, either already accessible from ARTIQ or made accessible with little effort.

Custom hardware components with widely extended capabilities and advanced support for scalable and fully distributed real-time control of experiments `are being designed <https://github.com/m-labs/artiq-hardware>`_.

ARTIQ and its dependencies are available in the form of `conda packages <https://conda.anaconda.org/m-labs/label/main>`_ for both Linux and Windows.
Packages containing pre-compiled binary images to be loaded onto the hardware platforms are supplied for each configuration.
Like any open source software ARTIQ can equally be built and installed directly from `source <https://github.com/m-labs/artiq>`_.

ARTIQ is supported by M-Labs and developed openly.
Components, features, fixes, improvements, and extensions are funded by and developed for the partnering research groups.

Technologies employed include `Python <https://www.python.org/>`_, `Migen <https://github.com/m-labs/migen>`_, `MiSoC <https://github.com/m-labs/misoc>`_/`mor1kx <https://github.com/openrisc/mor1kx>`_, `LLVM <http://llvm.org/>`_/`llvmlite <https://github.com/numba/llvmlite>`_, and `Qt5 <http://www.qt.io/>`_.

Website: https://m-labs.hk/artiq

Copyright (C) 2014-2016 M-Labs Limited. Licensed under GNU GPL version 3.
